Report form for late reported test results of **sample #20225**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Determination | Unit | Reference method \*) | Actual method used \*) | Unrounded  Result \*) | Rounded  result  *cfr.* used standard \*) |
| Total Acidity (Potentiometric) | mg KOH/g | EN62021-1 |  |  |  |
| Total Acidity (Colorimetric) | mg KOH/g | D974 |  |  |  |
| Appearance |  |  |  |  |  |
| Breakdown Voltage\*\*) | kV/2.5mm | EN60156 |  |  |  |
| Color ASTM |  | ISO2049 |  |  |  |
| Density at 20°C | kg/m3 | ISO3675 |  |  |  |
| Di-electric Dissipation Factor (DDF) measured at frequency: | | | \_\_\_\_\_\_\_\_\_\_ Hz | | |
| Di-electric Dissipation Factor (DDF) at 90°C |  | EN60247 |  |  |  |
| Specific Resistance at 90°C | GΩm | EN60247 |  |  |  |
| Flash Point C.O.C. | °C | D92 |  |  |  |
| Flash Point PMcc | °C | ISO2719-A |  |  |  |
| Interfacial Surface Tension | mN/m | D971 |  |  |  |
| Kinematic Viscosity at 40°C | mm2/s | D445 |  |  |  |
| Water | mg/kg | EN60814 |  |  |  |
| Additives | | | | | |
| - 2,6-Ditertiary-butyl phenol (DBP) | %M/M | D2668 |  |  |  |
| - 2,6-Ditertiary-butyl paracresol (DBPC) | %M/M | IEC60666 |  |  |  |
| - Dibenzyl disulfide (DBDS) | mg/kg | IEC62697 |  |  |  |
| - Benzotriazole (BTA) | mg/kg |  |  |  |  |
| - Irgamet 39 | mg/kg | Cigre WG A2.32 |  |  |  |

\*) Please see the letter of instructions before the start of the tests at [www.kpmd.co.uk/sgs-iis/](http://www.kpmd.co.uk/sgs-iis/)

\*\*) Please answer the additional questions about Breakdown Voltage if this determination is performed

**Please see the next page for the Additional Questions**

Report form for late reported test results

**Additional Questions**

**About Breakdown Voltage Determination**

1. Did you stirr during the determination of the Breakdown Voltage?

* Yes
* No

1. Remarks on Additional Questions:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_