Report form for late reported test results of **sample** **#21005**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Determination | unit | Reference method \*) | Actual method used \*) | ’Unrounded’result \*) | ’Rounded’result*cfr.* used standard \*) |
| Total Acid Number | mg KOH/g | D974 |  |  |  |
| Ash content | %M/M | ISO6245 |  |  |  |
| Calculated Cetane Index, four variables |  | ISO4264 |  |  |  |
| Cloud Point | °C | EN23015 |  |  |  |
| Cold Filter Plugging Point (CFPP) | °C | EN116 |  |  |  |
| Carbon Residue (Micro method) on 10% residue  | %M/M | ISO10370 |  |  |  |
| Copper Corrosion 3hrs at 50°C | rating |  |  |  |  |
| Density at 15°C | kg/m3 | ISO12185 |  |  |  |
| Distillation at 760 mmHg | **Manual or Automatic M / A\*\*)** |
| Initial Boiling Point | °C | ISO3405 |  |  |  |
| Temp at 10% recovered | °C | ISO3405 |  |  |  |
| Temp at 50% recovered | °C | ISO3405 |  |  |  |
| Temp at 90% recovered | °C | ISO3405 |  |  |  |
| Temp at 95% recovered | °C | ISO3405 |  |  |  |
| Final Boiling Point | °C | ISO3405 |  |  |  |
| Volume at 250°C | %V/V | ISO3405 |  |  |  |
| Volume at 350°C | %V/V | ISO3405 |  |  |  |
| FAME content | %V/V | EN14078 |  |  |  |
| Flash Point PMcc | °C | ISO2719-A |  |  |  |

\*) Please see the letter of instructions before the start of the tests at [www.kpmd.co.uk/sgs-iis/](http://www.kpmd.co.uk/sgs-iis/)

\*\*) Please circle the right option

**This table continues on the next page**

Report form for late reported test results of **sample** **#21005 – continued**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Determination | unit | Reference method \*) | Actual method used \*) | ’Unrounded’result \*) | ’Rounded’result*cfr.* used standard \*) |
| Kinematic Viscosity at 40°C | mm2/s | ISO3104 |  |  |  |
| Lubricity by HFRR at 60°C | µm | ISO12156-1 meth A |  |  |  |
| Was Lubricity by HFRR corrected or not? | **Corrected? Yes / No \*\*)** |
| Manganese as Mn | mg/L | EN16576 |  |  |  |
| Nitrogen \*\*\*) | mg/kg | D4629 |  |  |  |
| Polycyclic Aromatic Hydrocarbons 1) | %M/M | EN12916 |  |  |  |
| Mono-Aromatic Hydrocarbons | %M/M | EN12916 |  |  |  |
| Di-Aromatic Hydrocarbons | %M/M | EN12916 |  |  |  |
| Tri+-Aromatic Hydrocarbons | %M/M | EN12916 |  |  |  |
| Total Aromatic Hydrocarbons | %M/M | EN12916 |  |  |  |
| Pour Point Manual | °C | ISO3016 |  |  |  |
| Pour Point Automated 3°C interval | °C | D5950 |  |  |  |
| Sulfur | mg/kg | ISO20846 |  |  |  |
| Water  | mg/kg | ISO12937 |  |  |  |

\*) Please see the letter of instructions before the start of the tests at [www.kpmd.co.uk/sgs-iis/](http://www.kpmd.co.uk/sgs-iis/)

\*\*) Please circle the right option

\*\*\*)Please answer the additional questions about Nitrogen.

1) **Definition from EN12916:**

**%Polycyclic Aromatic Hydrocarbons = sum of %di- and %tri+-Aromatic Hydrocarbons**

**Additional Questions about Nitrogen:**

1. What Temperature in °C was used for the determination of the density of the sample (used to calculate the Nitrogen content of the sample in mg/kg)?

2. Remarks on Additional Questions: