Report form for late reported test results of **sample #22240, grade 35/50**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Determination | Unit | Reference method \*) | Actual method used \*) | UnroundedResult \*) | Roundedresult*cfr.* used standard \*) |
| Density at 25 °C | kg/m3 | EN15326 |  |  |  |
| Dynamic Viscosity at 60 °C | Pa.s | EN12596 |  |  |  |
| **Flash Point C.O.C.** | **method/procedure used: manual or automated \*\*)**  |
| Flash Point C.O.C. | °C | ISO2592 |  |  |  |
| **Fraass Breaking Point** | **method/procedure used EN12593:**  **manual or semi-automated or automated \*\*)**  |
| Fraass Breaking Point | °C | EN12593 |  |  |  |
| Kinematic Viscosity at 135 °C | mm2/s | EN12595 |  |  |  |
| **Penetration at 25 °C** | **method/procedure used: manual or automated \*\*)**  |
| Penetration at 25 °C  | 0.1 mm  | EN1426 |  |  |  |
| Penetration Index |  | EN12591 |  |  |  |
| **RTFOT at 163 °C** |  |
| Change of Mass | % | EN12607-1 |  |  |  |
| Retained Penetration | % | EN12607-1 |  |  |  |
| Viscosity Ratio |  | EN12607-1 |  |  |  |
| Increase in Softening Point | °C | EN12607-1 |  |  |  |
| Softening Point (Ring and Ball) | °C | EN1427 |  |  |  |
| Solubility in Xylene | %M/M | EN12592 |  |  |  |
| Ductility | cm | D113 |  |  |  |

\*) Please see the letter of instructions before the start of the tests at [www.kpmd.co.uk/sgs-iis/](http://www.kpmd.co.uk/sgs-iis/)

\*\*) Please circle the right option