Report form for late reported test results of **sample #21075**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Determination | Unit | Reference method \*) | Actual method used \*) | Unrounded  Result \*) | Rounded  result  *cfr.* used standard \*) |
| Total Acid Number \*\*\*) | mg KOH/g | D664-A |  |  |  |
| **Base Number** | **procedure used:**  **A forward, A back, B forward or B back \*\*)** | | | | |
| Base Number (HClO4 titration) | mg KOH/g | D2896 |  |  |  |
| Color ASTM |  | D1500 |  |  |  |
| Conradson Carbon Residue | %M/M | D189 |  |  |  |
| Ramsbottom Carbon Residue | %M/M | D524 |  |  |  |
| Carbon Residue (Micro method) | %M/M | D4530 |  |  |  |
| Density at 15°C | kg/L | ISO12185 |  |  |  |
| **Evaporation loss by Noack** | **procedure used: A, B, C, or D \*\*)** | | | | |
| Evaporation loss by Noack | %M/M | D5800 |  |  |  |
| Flash Point C.O.C. | °C | D92 |  |  |  |
| **Flash Point PMcc** | **procedure used: A or B \*\*)** | | | | |
| Flash Point PMcc | °C | D93 |  |  |  |
| **Foaming Tendency \*\*\*)** |  | | | | |
| Sequence I (5 min. blowing period) | mL | D892 |  |  |  |
| Sequence II (5 min. blowing period) | mL | D892 |  |  |  |
| Sequence III (5 min. blowing period) | mL | D892 |  |  |  |
| **Foam Stability \*\*\*)** |  | | | | |
| Sequence I (10 min. settling point) | mL | D892 |  |  |  |
| Sequence II (10 min. settling point) | mL | D892 |  |  |  |
| Sequence III (10 min. settling point) | mL | D892 |  |  |  |

\*) Please see the letter of instructions before the start of the tests at [www.kpmd.co.uk/sgs-iis/](http://www.kpmd.co.uk/sgs-iis/)

\*\*) Please circle the right option

\*\*\*) Please answer the additional questions about Total Acid Number (ASTM D664) and/or Foaming Characteristics if the determination is performed (see Additional Questions on the final page)

**This table continues on the next page.**

Report form for late reported test results of **sample** **#21075 - continued**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Determination | Unit | Reference method \*) | Actual method used \*) | Unrounded  Result \*) | Rounded  result  *cfr.* used standard \*) |
| Kinematic Viscosity at 40°C | mm2/s | D445 |  |  |  |
| Kinematic Viscosity at 100°C | mm2/s | D445 |  |  |  |
| Viscosity Index |  | D2270 |  |  |  |
| Viscosity Stabinger at 40°C | mm2/s | D7042 |  |  |  |
| Viscosity Stabinger at 100°C | mm2/s | D7042 |  |  |  |
| Viscosity HTHS | mPa.s | D4683 |  |  |  |
| Nitrogen | mg/kg | D5762 |  |  |  |
| Pour Point Manual | °C | D97 |  |  |  |
| Pour Point Automated 1°C interval | °C | D5950 |  |  |  |
| Sulfated Ash | %M/M | D874 |  |  |  |
| Sulfur | mg/kg | D4294 |  |  |  |
| **Water** | **procedure used: A, B or C \*\*)** | | | | |
| Water | mg/kg | D6304 |  |  |  |
| **Elemental Analyzes** |  | | | | |
| Calcium as Ca | mg/kg | D5185 |  |  |  |
| Phosphorus as P | mg/kg | D5185 |  |  |  |
| Zinc as Zn | mg/kg | D5185 |  |  |  |

\*) Please see the letter of instructions before the start of the tests at [www.kpmd.co.uk/sgs-iis/](http://www.kpmd.co.uk/sgs-iis/)

\*\*) Please circle the right option

**Please see the next page for the Additional Questions.**

Report form for late reported test results

**Additional Questions**

**About Total Acid Number (ASTM D664):**

What was the volume of the titration solvent?

* 60 mL
* 125 mL

How was the end point determined?

* Inflection Point
* Buffer End Point (pH 10)
* Buffer End Point (pH 11)

**About Foaming Characteristics:**

How was the sample used?

* As received
* After agitation (option A)
* Other, please specify below:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

What type of diffuser was used?

* Metal (Stainless Steel)
* Stone (Non-Metallic)

Remarks on Additional Questions:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_