Report form for late reported test results

**Please note that the sample is grinded and packed in vacuum.**

**Please do not age nor dry the sample before the test, nor determine volatile matter!**

**To ensure the homogeneity, please do not use less than 0.5 gram per determination.**

**For calculations please see the letter of instructions.**

**Sample #22540: gray grinded leather, approximately 5 grams**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Determination  | Unit | Referencemethod \*) | Actual method used \*) | ’Unrounded’result \*) | Roundedresult *cfr.* used standard \*) |
| Chromium (VI) (colorimetric) | mg/kg | ISO17075-1 |  |  |  |
| Chromium (VI) (chromatographic) | mg/kg  | ISO17075-2 |  |  |  |

\*) Please see the letter of instructions before the start of the tests at [www.kpmd.co.uk/sgs-iis-cts/](http://www.kpmd.co.uk/sgs-iis-cts/)

**Additional Questions**

1. Is your laboratory accredited in accordance with ISO/IEC17025 to determine the reported component(s)?

0 No

0 Yes

1. How many grams of sample intake was used? \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_
2. What was the time period in minutes between opening of the vacuum packed sample and extraction of the sample?

4. What was the pH of the **extraction solution** before extraction? \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

5. What was the pH of the **extraction solution** after extraction? \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

6. Remarks on Additional Questions: